Raspberry Pi bareback LF/MF/HF/VHF WSPR transmitter

Makes a very simple WSPR beacon from your RasberryPi by connecting GPIO
port to Antenna (and LPF), operates on LF, MF, HF and VHF bands from
0 to 250 MHz.

It is now compatible with both the original Raspberry Pi and the Raspberry Pi 2.

******
Installation / update:
******
  Make sure you are using the latest kernel by updating your system. The latest
  kernel includes fixes wich improve NTP ppm measurement accuracy:
    sudo apt-get update
    sudo apt-get dist-upgrade

  Download and compile code:
    sudo apt-get install git
    git clone https://github.com/JamesP6000/WsprryPi.git
    cd WsprryPi
    make

  See the accompanying BUILD file for more details.

******
Usage: (WSPR --help output):
******
  Usage:
    wspr [options] callsign locator tx_pwr_dBm f1 <f2> <f3> ...
      OR
    wspr [options] --test-tone f

  Options:
    -h --help
      Print out this help screen.
    -p --ppm ppm
      Known PPM correction to 19.2MHz RPi nominal crystal frequency.
    -s --self-calibration
      Call ntp_adjtime() before every transmission to obtain the PPM error of the xtal.
    -r --repeat
      Repeatedly, and in order, transmit on all the specified freqs.
    -x --terminate <n>
      Terminate after n transmissions have been completed.
    -o --offset
      Add a random frequency offset to each transmission:
        +/- 80 Hz for WSPR
        +/- 8 Hz for WSPR-15
    -t --test-tone freq
      Simply output a test tone and the specified frequency. Only used
      for debugging and to verify calibration.
    -n --no-delay
      Transmit immediately, do not wait for a WSPR TX window. Used
      for testing only.

  Frequencies can be specified either as an absolute TX carrier frequency, or
  using one of the following strings. If a string is used, the transmission
  will happen in the middle of the WSPR region of the selected band.
    LF LF-15 MF MF-15 160m 160m-15 80m 60m 40m 30m 20m 17m 15m 12m 10m 6m 4m 2m
  <B>-15 indicates the WSPR-15 region of band <B>.

  Transmission gaps can be created by specifying a TX frequency of 0
  
  Note that 'callsign', 'locator', and 'tx_power_dBm' are simply used to fill
  in the appropriate fields of the WSPR message. Normally, tx_power_dBm should
  be 10, representing the signal power coming out of the Pi. Set this value
  appropriately if you are using an external amplifier.

******
Radio licensing / RF:
******
  In order to transmit legally, a HAM Radio License is REQUIRED for running
  this experiment. The output is a square wave so a low pass filter is REQUIRED.
  Connect a low-pass filter (via decoupling C) to GPIO4 (GPCLK0) and Ground pin
  of your Raspberry Pi, connect an antenna to the LPF. The GPIO4 and GND pins
  are found on header P1 pin 7 and 9 respectively, the pin closest to P1 label
  is pin 1 and its 3rd and 4th neighbour is pin 7 and 9 respectively. See this
  link for pin layout: http://elinux.org/RPi_Low-level_peripherals Examples of
  low-pass filters can be found here: http://www.gqrp.com/harmonic_filters.pdf

  The expected power output is 10mW (+10dBm) in a 50 Ohm load. This looks
  neglible, but when connected to a simple dipole antenna this may result in
  reception reports ranging up to several thousands of kilometers.

  As the Raspberry Pi does not attenuate ripple and noise components from the
  5V USB power supply, it is RECOMMENDED to use a regulated supply that has
  sufficient ripple supression. Supply ripple might be seen as mixing products
  products centered around the transmit carrier typically at 100/120Hz.

  DO NOT expose GPIO4 to voltages or currents that are above the specified
  Absolute Maximum limits. GPIO4 outputs a digital clock in 3V3 logic, with a
  maximum current of 16mA. As there is no current protection available and a DC
  component of 1.6V, DO NOT short-circuit or place a resistive (dummy) load
  straight on the GPIO4 pin, as it may draw too much current. Instead, use a
  decoupling capacitor to remove DC component when connecting the output dummy
  loads, transformers, antennas, etc. DO NOT expose GPIO4 to electro- static
  voltages or voltages exceeding the 0 to 3.3V logic range; connecting an
  antenna directly to GPIO4 may damage your RPi due to transient voltages such
  as lightning or static buildup as well as RF from other transmitters
  operating into nearby antennas. Therefore it is RECOMMENDED to add some form
  of isolation, e.g. by using a RF transformer, a simple buffer/driver/PA
  stage, two schottky small signal diodes back to back.

******
TX Timing:
******
  This software is using system time to determine the start of WSPR
  transmissions, so keep the system time synchronised within 1sec precision,
  i.e. use NTP network time synchronisation or set time manually with date
  command. A WSPR broadcast starts on an even minute and takes 2 minutes for
  WSPR-2 or starts at :00,:15,:30,:45 and takes 15 minutes for WSPR-15. It
  contains a callsign, 4-digit Maidenhead square locator and transmission
  power.  Reception reports can be viewed on Weak Signal Propagation Reporter
  Network at: http://wsprnet.org/drupal/wsprnet/spots

******
Calibration:
******
  Frequency calibration is REQUIRED to ensure that the WSPR-2 transmission
  occurs within the narrow 200 Hz band. The reference crystal on your RPi might
  have an frequency error (which in addition is temp. dependent -1.3Hz/degC
  @10MHz). To calibrate, the frequency might be manually corrected on the
  command line or a PPM correction could be specified on the command line.

  NTP calibration:
  NTP automatically tracks and calculates a PPM frequency correction. If you
  are running NTP on your Pi, you can use the --self-calibration option to
  have this program querry NTP for the latest frequency correction before
  each WSPR transmission. Some residual frequency error may still be present
  due to delays in the NTP measurement loop and this method works best if your
  Pi has been on for a long time, the crystal's temperature has stabilized,
  and the NTP control loop has converged.

  AM calibration:
  A practical way to calibrate is to tune the transmitter on the same frequency
  of a medium wave AM broadcast station; keep tuning until zero beat (the
  constant audio tone disappears when the transmitter is exactly on the same
  frequency as the broadcast station), and determine the frequency difference
  with the broadcast station. This is the frequency error that can be applied
  for correction while tuning on a WSPR frequency.

  Suppose your local AM radio station is at 780kHz. Use the --test-tone option
  to produce different tones around 780kHz (eg 780100 Hz) until you can
  successfully zero beat the AM station. If the zero beat tone specified on the
  command line is F, calculate the PPM correction required as:
  ppm=(F/780000-1)*1e6 In the future, specify this value as the argument to the
  --ppm option on the comman line. You can verify that the ppm value has been
  set correction by specifying --test-tone 780000 --ppm <ppm> on the command
  line and confirming that the Pi is still zero beating the AM station.

******
PWM Peripheral:
******
  The code uses the RPi PWM peripheral to time the frequency transitions
  of the output clock. This peripheral is also used by the RPi sound system
  and hence any sound events that occur during a WSPR transmission will
  interfere with WSPR transmissions. Sound can be permanently disabled
  by editing /etc/modules and commenting out the snd-bcm2835 device.

******
Example usage:
******
  Brief help screen
    ./wspr --help

  Transmit a constant test tone at 780 kHz.
    sudo ./wspr --test-tone 780e3

  Using callsign N9NNN, locator EM10, and TX power 33 dBm, transmit a single
  WSPR transmission on the 20m band using NTP based frequency offset
  calibration.
    sudo ./wspr --self-calibration N9NNN EM10 33 20m

  Transmit a WSPR transmission slightly off-center on 30m every 10 minutes for
  a total of 7 transmissions, and using a fixed PPM correction value.  sudo
    sudo ./wspr --repeat --terminate 7 --ppm 43.17 N9NNN EM10 33 10140210 0 0 0 0

  Transmit repeatedly on 40m, use NTP based frequency offset calibration,
  and add a random frequency offset to each transmission to minimize collisions
  with other transmissions.
    sudo ./wspr --repeat --offset --self-calibration N9NNN EM10 33 40m

******
Reference documentation:
******
  http://www.raspberrypi.org/wp-content/uploads/2012/02/BCM2835-ARM-Peripherals.pdf
  http://www.scribd.com/doc/127599939/BCM2835-Audio-clocks
  http://www.scribd.com/doc/101830961/GPIO-Pads-Control2
  https://github.com/mgottschlag/vctools/blob/master/vcdb/cm.yaml
  https://www.kernel.org/doc/Documentation/vm/pagemap.txt

******
Credits:
******
  Credits goes to Oliver Mattos and Oskar Weigl who implemented PiFM [1]
  based on the idea of exploiting RPi DPLL as FM transmitter.

  Dan MD1CLV combined this effort with WSPR encoding algorithm from F8CHK,
  resulting in WsprryPi a WSPR beacon for LF and MF bands.

  Guido PE1NNZ <pe1nnz@amsat.org> extended this effort with DMA based PWM
  modulation of fractional divider that was part of PiFM, allowing to operate
  the WSPR beacon also on HF and VHF bands.  In addition time-synchronisation
  and double amount of power output was implemented.

  James Peroulas <james@peroulas.com> added several command line options, a
  makefile, improved frequency generation precision so as to be able to
  precisely generate a tone at a fraction of a Hz, and added a self calibration
  feature where the code attempts to derrive frequency calibration information
  from an installed NTP deamon.  Furthermore, the TX length of the WSPR symbols
  is more precise and does not vary based on system load or PWM clock
  frequency.

  Michael Tatarinov for adding a patch to get PPM info directly from the
  kernel.

  [1] PiFM code from
      http://www.icrobotics.co.uk/wiki/index.php/Turning_the_Raspberry_Pi_Into_an_FM_Transmitter
  [2] Original WSPR Pi transmitter code by Dan:
      https://github.com/DanAnkers/WsprryPi
  [3] Fork created by Guido:
      https://github.com/threeme3/WsprryPi
  [4] This fork created by James:
      https://github.com/JamesP6000/WsprryPi

